InS_StArT
NE1500T.COM
1.0
^Novell Ethernet NE1500T,NE1500T.COM,IE0
^Ansel M1500,NE1500T.COM,IE0
?Only one NE1500T can be installed in a machine and it must be in a 16 bit expansion slot.
!RIE0(INT)Hardware Interrupt
@3
4
5
9
!RIE0(PORT)Base I/O Port
@300
320
340
360
!RIE0(DMA)DMA Channel
3
@5
6
7
$OIE0(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
