InS_StArT
DC21040.COM
1.0
^Linksys EtherPCI,DC21040.COM,IE0
?Please select the options that match your board's jumper settings.
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
@Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
