InS_StArT
NE2_32.COM
1.0
^Novell/Eagle NE2-32,NE2_32.COM,00M,7151
?Please select the options that match your board's jumper settings.
!R00M(INT)Hardware Interrupt
2
@3
4
5
9
10
11
!R00M(PORT)Base I/O Port
@3000
4000
5000
6000
7000
9000
D000
!RIEM(MEM)Base Memory
@000C0000
000D0000
FFF90000
FFFA0000
FFFB0000
FFFC0000
FFFD0000
!R00M(SLOT)Slot
1
2
3
4
5
6
7
8
$O00M(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*R00M(FRAME)Media Frame Type
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@ETHERNET_802.2
ETHERNET_802.3
ETHERNET_II
ETHERNET_SNAP
InS_EnD
