== RIO mash test :: COM1 @ 62500 8N1, 300s, chip label 'patched-62500-retx' ==
   lamp echo ON (drives reply/lamp collisions), wedge threshold 2.0s, app auto-recovery DISABLED
   log: C:\VWE\riojoy\riomash-patched-62500-retx-20260719-131037.log
   firmware: 4.2
   counters before: RestartCount=0  AbandonCount=0  FullBufferCount=0  [board/lamp faults reported!]

>>> MASH NOW: two hands, 8 lamp buttons, as fast as you can. <<<
>>> Test runs 300s. A wedge alarm will beep + banner.   <<<
>>> Ctrl+C ends the run early and still prints the summary.   <<<

[  33.03s] progress: presses=245 (245/min) analog=515 maxGap=0.27s wedges=0
[  63.05s] progress: presses=568 (541/min) analog=992 maxGap=0.27s wedges=0
[  93.11s] progress: presses=709 (457/min) analog=1470 maxGap=0.27s wedges=0
[  95.30s] operator stop (Ctrl+C) — ending run, snapshotting counters...

== MASH SUMMARY [patched-62500-retx] ==
run              : 95s on COM1, lamps on, wedge threshold 2.0s
firmware         : 4.2
presses/releases : 709 / 710  (440 presses/min)
analog replies   : 1522 (~1727 poll slots; 88.1%), sentinels 0
framing / NAK    : 61 / 321 (NAK-triggered resends: 321)
gap histogram    : <100ms:1510  100-250ms:9  250-500ms:2  0.5-1s:0  1-2s:0  2-5s:0  >5s:0
longest gaps     : 0.27s@1.8s, 0.25s@95.3s, 0.13s@77.1s, 0.13s@26.6s, 0.12s@26.3s, 0.12s@57.4s, 0.12s@12.7s, 0.12s@11.5s, 0.12s@18.8s, 0.12s@31.3s
wedge events     : 0
counters before  : RestartCount=0  AbandonCount=0  FullBufferCount=0  [board/lamp faults reported!]
counters after   : RestartCount=0  AbandonCount=0  FullBufferCount=0  [board/lamp faults reported!]
counter delta    : RestartCount=+0  AbandonCount=+0  FullBufferCount=+0
verdict          : PASS — no wedge; compare gap histogram + counter delta to baseline
log file         : C:\VWE\riojoy\riomash-patched-62500-retx-20260719-131037.log
