== RIO mash test :: COM1 @ 62500 8N1, 300s, chip label 'patched-62500-sw' ==
   lamp echo ON (drives reply/lamp collisions), wedge threshold 2.0s, app auto-recovery DISABLED
   log: C:\VWE\riojoy\riomash-patched-62500-sw-20260719-133628.log
   firmware: 4.2
   counters before: RestartCount=0  AbandonCount=0  FullBufferCount=0  [board/lamp faults reported!]

>>> MASH NOW: two hands, 8 lamp buttons, as fast as you can. <<<
>>> Test runs 300s. A wedge alarm will beep + banner.   <<<
>>> Ctrl+C ends the run early and still prints the summary.   <<<

[  31.90s] progress: presses=72 (72/min) analog=497 maxGap=0.21s wedges=0
[  58.27s] operator stop (Ctrl+C) — ending run, snapshotting counters...

== MASH SUMMARY [patched-62500-sw] ==
run              : 58s on COM1, lamps on, wedge threshold 2.0s
firmware         : 4.2
presses/releases : 123 / 123  (124 presses/min)
analog replies   : 931 (~1054 poll slots; 88.3%), sentinels 0
framing / NAK    : 7 / 20 (command resends NAK/timeout: 34)
gap histogram    : <100ms:921  100-250ms:9  250-500ms:0  0.5-1s:0  1-2s:0  2-5s:0  >5s:0
longest gaps     : 0.22s@58.3s, 0.21s@0.6s, 0.14s@41.9s, 0.14s@26.8s, 0.13s@23.6s, 0.11s@12.4s, 0.11s@24.4s, 0.10s@54.1s, 0.10s@53.4s, 0.10s@16.5s
wedge events     : 0
counters before  : RestartCount=0  AbandonCount=0  FullBufferCount=0  [board/lamp faults reported!]
counters after   : RestartCount=0  AbandonCount=0  FullBufferCount=0  [board/lamp faults reported!]
counter delta    : RestartCount=+0  AbandonCount=+0  FullBufferCount=+0
verdict          : PASS — no wedge; compare gap histogram + counter delta to baseline
log file         : C:\VWE\riojoy\riomash-patched-62500-sw-20260719-133628.log
